may 14,1996 modified: august 26,1997

Proposal for the Straw Tube Readout Channels and cables numbering scheme

L. Benussi, M.Bertani, S.Bianco, L.Passamonti

1 Readout Channels and cables numbering scheme

Each cable/channel is identified by a code DDTTWWWW, where:

ffl DD (A-Z) Detector code;

ffl TT (A-Z) Module type of detector DD;

ffl WWWW number of either type: XYYY with X=1:9 and YYY=1:999, or

XXYY with XX=1:99 and YY=1:99 identifying respectivly the cable number and the channel number in the cable.

For example, the Straw tube detector DD=ST has the numbering scheme shown in table (tab.1). This is a general numbering scheme followed by all the detectors [1].

Table 1: Numbering scheme for readout channels and cables for the Straw Tubes detector.

description (DDTTWWWW) comment straw tube STSTXYYY layer X=1 � 6, tube YYY=001 � 404 from straw to Patch Panel STSPXYYY same from Patch Panel to Disc STPDX0YY layer X=1 � 6, cable YY=01 � 14 from Disc to TDC STDTX0YY same High Voltage to Patch Panel STHPX0YY same Low Voltage to Patch Panel STLPX0YY same Test Pulse cable STTPX0YY same gas cable STGAX0YZ layer X=1 � 6, Y=1(input), 2(output), distributor Z=1 � 7

References

[1] S.Bianco, A. Cecchetti, Finuda Note 34/lnf/opr/96

1